**Inhaltsverzeichnis: Ausschreibungstexte Aliaxis Deutschland GmbH  
FRIAMAT Schweißgeräte**

**1.0 FRIAMAT prime eco**

**2.0** **FRIAMAT basic eco**

**3.0** **FRIAMAT 7 prime**

**4.0** **FRIAMAT 7 basic**

**Table of Contents: Tendering Text Aliaxis Deutschland GmbH  
FRIAMAT Fusion units**

**1.0 FRIAMAT prime eco**

**2.0** **FRIAMAT basic eco**

**3.0** **FRIAMAT 7 prime**

**4.0** **FRIAMAT 7 basic**

**5.0** **FRIAMAT 6 110V**

**Ausschreibungstexte** FRIAMAT**-Schweißgeräte**

**Aliaxis Deutschland GmbH Mannheim, Infrastruktur,** [**www.aliaxis.de**](http://www.aliaxis.de)**, Tel.: (0621) 486 - 0**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Pos.** | **Anzahl** | **Text** | **EP** | **GP** |
| 1.0 |  | **FRIAMAT prime eco**  **Schweißgerät mit Dokumentationsfunktion**  **Leistungsstarkes Universal-Schweißgerät FRIAMAT prime eco**  Merkmale:   * Bluetooth * Volle Dokumentation * Volle Traceabilityfunktionen * 20.000 Schweißprotokolle * Ausgabe über USB-Schnittstelle oder App (Smartphone) * Supervisorfunktion * Ringkerntechnologie mit aktiver Kühlung * Helles TFT-Farbdisplay * Mit Mini-Scanner oder 1D/2D-Scanner (2D Barcodes nach ISO 12176-5) * Extra langes Schweißkabel (4 m) * Extra langes Netzkabel (5 m) * Gewicht ca. 18,0 kg * Möglichkeit der Aktualisierung der FRIAMAT Software über die USB-Schnittstelle durch den Anwender |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Pos.** | **Anzahl** | **Text** | **EP** | **GP** |
| 2.0 |  | **FRIAMAT basic eco**  **Schweißgerät ohne Dokumentationsfunktion**  **Leistungsstarkes Universal-Schweißgerät FRIAMAT basic eco**  Merkmale:   * Ringkerntechnologie mit aktiver Kühlung * Helles TFT-Farbdisplay * Mit Mini-Scanner oder 1D/2D-Scanner (2D Barcodes nach ISO 12176-5) * Extra langes Schweißkabel (4 m) * Extra langes Netzkabel (5 m) * Gewicht ca. 18,0 kg * Möglichkeit der Aktualisierung der FRIAMAT Software über die USB-Schnittstelle durch den Anwender |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Pos.** | **Anzahl** | **Text** | **EP** | **GP** |
| 3.0 |  | **FRIAMAT 7 prime**  **Schweißgerät mit Dokumentationsfunktion**  **Leistungsstarkes Universal-Schweißgerät FRIAMAT 7 prime**  Merkmale:   * Bluetooth * Volle Dokumentation * Volle Traceabilityfunktionen * 20.000 Schweißprotokolle * Ausgabe über USB-Schnittstelle oder App (Smartphone) * Supervisorfunktion * Modernste Konvertertechnologie mit aktiver Kühlung * Helles TFT-Farbdisplay * Mit Mini-Scanner oder 1D/2D-Scanner (2D Barcodes nach ISO 12176-5) * Extra langes Schweißkabel (4 m) * Extra langes Netzkabel (5 m) * Gewicht ca. 12,8 kg * Möglichkeit der Aktualisierung der FRIAMAT Software über die USB-Schnittstelle durch den Anwender |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Pos.** | **Anzahl** | **Text** | **EP** | **GP** |
| 4.0 |  | **FRIAMAT 7 basic**  **Schweißgerät ohne Dokumentationsfunktion**  **Leistungsstarkes Universal-Schweißgerät FRIAMAT 7 basic**  Merkmale:   * Modernste Konvertertechnologie mit aktiver Kühlung * Helles TFT-Farbdisplay * Mit Mini-Scanner oder 1D/2D-Scanner (2D Barcodes nach ISO 12176-5) * Extra langes Schweißkabel (4 m) * Extra langes Netzkabel (5 m) * Gewicht ca. 12,8 kg * Möglichkeit der Aktualisierung der FRIAMAT Software über die USB-Schnittstelle durch den Anwender |  |  |

**Tendering Texts for** FRIAMAT **Fusion units**

**Aliaxis Deutschland GmbH Mannheim, Germany, Infrastructure,** [**www.aliaxis.de**](http://www.aliaxis.de)**/en**

**Tel.: +49 621 486 - 0**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Item** | **Qty.** | **Text** | **UP** | **TP** |
| 1.0 |  | **FRIAMAT prime eco**  **Fusion unit with documentation function**  **Powerful universal fusion unit FRIAMAT prime eco**  Features:   * Bluetooth * Full documentation * Full traceability functions * 20,000 fusion protocols * Output via USB interface or app (smart phone) * Supervisor function * Toroidal core technology with active cooling * Bright colour TFT display * With mini scanner or 1D/2D scanner (2D barcodes according to ISO 12176-5) * Extra long fusion cable (4 m) * Extra long power cable (5 m) * Weight approx. 18.0 kg * Possibility of updating the FRIAMAT software via the USB-interface by the user |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Item** | **Qty.** | **Text** | **UP** | **TP** |
| 2.0 |  | **FRIAMAT basic eco**  **Fusion unit without documentation function**  **Powerful universal fusion unit FRIAMAT basic eco**  Features:   * Toroidal transformer technology with active cooling * Bright colour TFT display * With mini-scanner or 1D/2D scanner (2D barcodes according to ISO 12176-5) * Extra long fusion cable (4 m) * Extra long power cable (5 m) * Weight approx. 18.0 kg * Possibility of updating the FRIAMAT software via the USB-interface by the user |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Item** | **Qty.** | **Text** | **UP** | **TP** |
| 3.0 |  | **FRIAMAT 7 prime**  **Fusion unit with documentation function**  **Powerful universal fusion unit FRIAMAT 7 prime**  Features:   * Bluetooth * Full documentation * Full traceability functions * 20,000 fusion protocols * Output via USB interface or app (smart phone) * Supervisor function * State-of-the-art converter technology with active cooling * Bright colour TFT display * With mini scanner or 1D/2D scanner (2D barcodes according to ISO 12176-5) * Extra long fusion cable (4 m) * Extra long power cable (5 m) * Weight approx. 12.8 kg * Possibility of updating the FRIAMAT software via the USB-interface by the user |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Item** | **Qty.** | **Text** | **UP** | **TP** |
| 4.0 |  | **FRIAMAT 7 basic**  **Fusion unit without documentation function**  **Powerful universal fusion unit FRIAMAT 7 basic**  Features:   * State-of-the-art converter technology with active cooling * Bright colour TFT display * With mini scanner or 1D/2D scanner (2D barcodes according to ISO 12176-5) * Extra long fusion cable (4 m) * Extra long power cable (5 m) * Weight approx. 12.8 kg * Possibility of updating the FRIAMAT software via the USB-interface by the user |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Item** | **Qty.** | **Text** | **UP** | **TP** |
| 5.0 |  | **FRIAMAT 6 110V**  **Fusion unit with documentation function**  **Powerful universal fusion unit FRIAMAT 6 110V**  Features:   * Bluetooth * Full documentation * Full traceability functions * 20,000 fusion protocols * Output via USB-interface or app (smart phone) * Supervisor function * State-of-the-art toroidal core technology with active cooling * Bright colour TFT display * With mini scanner * Possibility of updating the FRIAMAT software via the USB-interface by the user * Other main plugs variants on request * 1D/2D scanner on request   **UK metric:**   * Extra long fusion cable (4 m) * Extra long power cable (5 m) * Weight approx. 19.0 kg   **US imperial:**   * Extra long fusion cable (13 ft) * Extra long power cable (16 ft) * Weight approx. 42 lbs |  |  |