**Inhaltsverzeichnis: Ausschreibungstexte Aliaxis Deutschland GmbH
FRIAMAT Schweißgeräte**

**1.0 FRIAMAT prime eco**

**2.0** **FRIAMAT basic eco**

**3.0** **FRIAMAT 7 prime**

**4.0** **FRIAMAT 7 basic**

**Table of Contents: Tendering Text Aliaxis Deutschland GmbH
FRIAMAT Fusion units**

**1.0 FRIAMAT prime eco**

**2.0** **FRIAMAT basic eco**

**3.0** **FRIAMAT 7 prime**

**4.0** **FRIAMAT 7 basic**

**5.0** **FRIAMAT 6 110V**

**Ausschreibungstexte** FRIAMAT**-Schweißgeräte**

**Aliaxis Deutschland GmbH Mannheim, Infrastruktur,** [**www.aliaxis.de**](http://www.aliaxis.de)**, Tel.: (0621) 486 - 0**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Pos.** | **Anzahl** | **Text** | **EP** | **GP** |
| 1.0  |  | **FRIAMAT prime eco****Schweißgerät mit Dokumentationsfunktion** **Leistungsstarkes Universal-Schweißgerät FRIAMAT prime eco**Merkmale:* Bluetooth
* Volle Dokumentation
* Volle Traceabilityfunktionen
* 20.000 Schweißprotokolle
* Ausgabe über USB-Schnittstelle oder App (Smartphone)
* Supervisorfunktion
* Ringkerntechnologie mit aktiver Kühlung
* Helles TFT-Farbdisplay
* Mit Mini-Scanner oder 1D/2D-Scanner (2D Barcodes nach ISO 12176-5)
* Extra langes Schweißkabel (4 m)
* Extra langes Netzkabel (5 m)
* Gewicht ca. 18,0 kg
* Möglichkeit der Aktualisierung der FRIAMAT Software über die USB-Schnittstelle durch den Anwender
 |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Pos.** | **Anzahl** | **Text** | **EP** | **GP** |
| 2.0 |  | **FRIAMAT basic eco****Schweißgerät ohne Dokumentationsfunktion** **Leistungsstarkes Universal-Schweißgerät FRIAMAT basic eco**Merkmale:* Ringkerntechnologie mit aktiver Kühlung
* Helles TFT-Farbdisplay
* Mit Mini-Scanner oder 1D/2D-Scanner (2D Barcodes nach ISO 12176-5)
* Extra langes Schweißkabel (4 m)
* Extra langes Netzkabel (5 m)
* Gewicht ca. 18,0 kg
* Möglichkeit der Aktualisierung der FRIAMAT Software über die USB-Schnittstelle durch den Anwender

 |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Pos.** | **Anzahl** | **Text** | **EP** | **GP** |
| 3.0 |  | **FRIAMAT 7 prime****Schweißgerät mit Dokumentationsfunktion** **Leistungsstarkes Universal-Schweißgerät FRIAMAT 7 prime**Merkmale:* Bluetooth
* Volle Dokumentation
* Volle Traceabilityfunktionen
* 20.000 Schweißprotokolle
* Ausgabe über USB-Schnittstelle oder App (Smartphone)
* Supervisorfunktion
* Modernste Konvertertechnologie mit aktiver Kühlung
* Helles TFT-Farbdisplay
* Mit Mini-Scanner oder 1D/2D-Scanner (2D Barcodes nach ISO 12176-5)
* Extra langes Schweißkabel (4 m)
* Extra langes Netzkabel (5 m)
* Gewicht ca. 12,8 kg
* Möglichkeit der Aktualisierung der FRIAMAT Software über die USB-Schnittstelle durch den Anwender

 |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Pos.** | **Anzahl** | **Text** | **EP** | **GP** |
| 4.0 |  | **FRIAMAT 7 basic****Schweißgerät ohne Dokumentationsfunktion** **Leistungsstarkes Universal-Schweißgerät FRIAMAT 7 basic**Merkmale:* Modernste Konvertertechnologie mit aktiver Kühlung
* Helles TFT-Farbdisplay
* Mit Mini-Scanner oder 1D/2D-Scanner (2D Barcodes nach ISO 12176-5)
* Extra langes Schweißkabel (4 m)
* Extra langes Netzkabel (5 m)
* Gewicht ca. 12,8 kg
* Möglichkeit der Aktualisierung der FRIAMAT Software über die USB-Schnittstelle durch den Anwender

 |  |  |

**Tendering Texts for** FRIAMAT **Fusion units**

**Aliaxis Deutschland GmbH Mannheim, Germany, Infrastructure,** [**www.aliaxis.de**](http://www.aliaxis.de)**/en**

**Tel.: +49 621 486 - 0**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Item** | **Qty.** | **Text** | **UP** | **TP** |
| 1.0  |  | **FRIAMAT prime eco****Fusion unit with documentation function** **Powerful universal fusion unit FRIAMAT prime eco**Features:* Bluetooth
* Full documentation
* Full traceability functions
* 20,000 fusion protocols
* Output via USB interface or app (smart phone)
* Supervisor function
* Toroidal core technology with active cooling
* Bright colour TFT display
* With mini scanner or 1D/2D scanner (2D barcodes according to ISO 12176-5)
* Extra long fusion cable (4 m)
* Extra long power cable (5 m)
* Weight approx. 18.0 kg
* Possibility of updating the FRIAMAT software via the USB-interface by the user
 |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Item** | **Qty.** | **Text** | **UP** | **TP** |
| 2.0  |  | **FRIAMAT basic eco****Fusion unit without documentation function** **Powerful universal fusion unit FRIAMAT basic eco**Features:* Toroidal transformer technology with active cooling
* Bright colour TFT display
* With mini-scanner or 1D/2D scanner (2D barcodes according to ISO 12176-5)
* Extra long fusion cable (4 m)
* Extra long power cable (5 m)
* Weight approx. 18.0 kg
* Possibility of updating the FRIAMAT software via the USB-interface by the user
 |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Item** | **Qty.** | **Text** | **UP** | **TP** |
| 3.0  |  | **FRIAMAT 7 prime** **Fusion unit with documentation function** **Powerful universal fusion unit FRIAMAT 7 prime** Features:* Bluetooth
* Full documentation
* Full traceability functions
* 20,000 fusion protocols
* Output via USB interface or app (smart phone)
* Supervisor function
* State-of-the-art converter technology with active cooling
* Bright colour TFT display
* With mini scanner or 1D/2D scanner (2D barcodes according to ISO 12176-5)
* Extra long fusion cable (4 m)
* Extra long power cable (5 m)
* Weight approx. 12.8 kg
* Possibility of updating the FRIAMAT software via the USB-interface by the user
 |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Item** | **Qty.** | **Text** | **UP** | **TP** |
| 4.0  |  | **FRIAMAT 7 basic** **Fusion unit without documentation function** **Powerful universal fusion unit FRIAMAT 7 basic** Features:* State-of-the-art converter technology with active cooling
* Bright colour TFT display
* With mini scanner or 1D/2D scanner (2D barcodes according to ISO 12176-5)
* Extra long fusion cable (4 m)
* Extra long power cable (5 m)
* Weight approx. 12.8 kg
* Possibility of updating the FRIAMAT software via the USB-interface by the user
 |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Item** | **Qty.** | **Text** | **UP** | **TP** |
| 5.0  |  | **FRIAMAT 6 110V** **Fusion unit with documentation function** **Powerful universal fusion unit FRIAMAT 6 110V** Features:* Bluetooth
* Full documentation
* Full traceability functions
* 20,000 fusion protocols
* Output via USB-interface or app (smart phone)
* Supervisor function
* State-of-the-art toroidal core technology with active cooling
* Bright colour TFT display
* With mini scanner
* Possibility of updating the FRIAMAT software via the USB-interface by the user
* Other main plugs variants on request
* 1D/2D scanner on request

**UK metric:*** Extra long fusion cable (4 m)
* Extra long power cable (5 m)
* Weight approx. 19.0 kg

**US imperial:*** Extra long fusion cable (13 ft)
* Extra long power cable (16 ft)
* Weight approx. 42 lbs
 |  |  |